For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the screws and the license plate lamp assembly.
3. Remove the bulb.

### Installation Procedure

1. Install the replacement bulb.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the license plate lamp assembly with the screws.

Tighten
Tighten the license plate lamp assembly screws to 4 N·m (35 lb in).

3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .