For 1990-2009 cars

## Steering Column Trim Cover Replacement C100/Long Body

### Removal Procedure

1. Remove the lower steering column cover screw.
2. Turn the steering wheel in order to expose the upper steering column cover screws. Remove the upper steering column cover screws and remove the upper steering column cover.
3. Remove the lower steering column cover from the cluster bezel.

### Installation Procedure

1. Install the lower steering column cover to the cluster bezel.
2. Install the upper steering column cover.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the upper and lower steering column cover screws and tighten to 1.5 N·m (13 lb in).

## Steering Column Trim Cover Replacement C105/Short Body

### Removal Procedure

1. Remove the lower steering column cover panel screw.
2. Turn the steering wheel in order to expose the upper steering column cover panel screws.
3. Remove the upper steering column cover panel screws.
4. Remove the upper steering column cover panel.
5. Remove the lower steering column cover panel from the cluster bezel.

### Installation Procedure

1. Install the lower steering column cover panel to the cluster bezel.
2. Install the upper steering column cover panel.
3. Turn the steering wheel in order to expose the upper steering column cover panel screw holes.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the upper and the lower steering column cover panel screws and tighten to 1.5 N·m (13 lb in).