For 1990-2009 cars

### Removal Procedure

1. Remove the door hold-open link-to-body bolt and the door hold-open link.
2. Remove the door weather strip.

### Installation Procedure

1. Install the door weather strip.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door hold-open link to the body with the bolt.

Tighten
Tighten the door hold-open link-to-body bolt to 20 N·m (15 lb ft).