For 1990-2009 cars

## Exhaust Muffler Replacement 2.0L Diesel

### Removal Procedure

Warning: In order to avoid being burned, do not service the exhaust system while it is still hot. Service the system when it is cool.

Caution: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

1. Remove the nuts and the gaskets from the both rear muffler pipe flange-to-front muffler pipe flange.
2. Detach the both rear muffler assembly from the rubber hangers.
3. Remove the both rear muffler.
4. Check the rear muffler and the pipe for holes, damage, open seams and other deterioration which could permit exhaust fumes to seep into the passenger compartment or the trunk.

### Installation Procedure

1. Secure the both rear muffler assembly to the rubber hangers.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and the gaskets to the both rear muffler pipe flange-to-front muffler pipe flange and tighten to 40 N·m (30 lb ft).

## Exhaust Muffler Replacement 2.4L

### Removal Procedure

1. Remove the nuts and the gaskets from both resonator pipe flanges-to-front muffler pipe flanges.
2. Detach both resonator assemblies from the rubber hangers.
3. Remove both resonators.
4. Check the rear resonator and the pipe for holes, damage, open seams and other deterioration which could permit exhaust fumes to seep into the passenger compartment or the trunk.

### Installation Procedure

1. Secure both rear resonator assemblies to the rubber hangers.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and the gaskets to both rear resonator pipe flanges-to-front muffler pipe flanges and tighten the nuts to 40 N·m (30 lb ft).

## Exhaust Muffler Replacement 3.2L

### Removal Procedure

1. Remove the nuts and the gaskets from the rear muffler pipe flange-to-front muffler pipe flange.
2. Detach the rear muffler assembly from the rubber hangers.
3. Remove the rear muffler.
4. Check the rear muffler and the pipe for holes, damage, open seams or other deterioration which could permit exhaust fumes to seep into the passenger compartment or the trunk.

### Installation Procedure

1. Secure the rear muffler assembly to the rubber hangers.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and the gaskets to the rear muffler pipe flange-to-front muffler pipe flange and tighten nuts to 40 N·m (30 lb ft).