For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Pull the relay straight up and out from its location in the engine fuse block at the left front corner.

### Installation Procedure

1. Align the relay terminal contacts with the base receptacle.
2. Push the relay into the base until it is seated.
3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .