For 1990-2009 cars

## Fastener Tightening Specifications 2.4L

Application | Specification
--- | ---
Metric | English
Fan Assembly Mounting Bolts | 4 N·m | 35 lb in
Fan Blade Retaining Nut | 5.6 N·m | 50 lb in
Fan Motor Retaining Screws | 3.5 N·m | 31 lb in
Radiator Upper Left and right Racket Retaining Bolts | 20 N·m | 15 lb ft
Surge Tank Mounting Bolt and Nut | 8 N·m | 71 lb in
Thermostat Housing Mounting Bolts | 15 N·m | 11 lb ft
Water Pump Mounting Bolts | 25 N·m | 18 lb ft

## Fastener Tightening Specifications 3.2L

Application | Specification
--- | ---
Metric | English
Condenser, Radiator, Fan Module (CRFM) Assembly Support Bracket Mounting Bolt | 50 N·m | 37 lb ft
CRFM Assembly Support Bracket Through Bolt and Nut | 50 N·m | 37 lb ft
Fan Assembly Mounting Bolts | 4 N·m | 35 lb in
Fan Blade Retaining Nut | 5.6 N·m | 50 lb in
Fan Motor Retaining Screws | 3.5 N·m | 31 lb in
Heater Inlet and Outlet Pipe Bracket Retaining Bolts | 12 N·m | 106 lb in
Radiator Upper Left and Right Bracket Retaining Bolts. | 20 N·m | 15 lb ft
Surge Tank Mounting Bolt and Nut | 8 N·m | 71 lb in
Thermostat Housing Mounting Bolts | 10 N·m | 89 lb in
Water Outlet Port Attaching Bolt | 10 N·m | 89 lb in
Water Pipe to Thermostat Housing Attaching Bolt | 20 N·m | 15 lb ft
Water Pipe to Cylinder Head Attaching Bolt | 33 N·m | 24 lb ft
Water Pump Mounting Bolts | 25 N·m | 18 lb ft
Water Pump Pulley Retaining Bolts | 12 N·m | 106 lb in

## Fastener Tightening Specifications 2.0L Diesel

Application | Specification
--- | ---
Metric | English
A/C Condensor Retaining Bolt | 16 N·m | 11.8 lb ft
Cooling Fan Assembly Bolt | 4 N·m | 35 lb in
Fan Blades Retaining Screw | 5.6 N·m | 35 lb in
Fan Motor Retaining Screw | 3.5 N·m | 50 lb in
Radiator Lower Bracket Bolt | 50 N·m | 31 lb ft
Radiator Upper Bracket Retaining Bolt | 20 N·m | 36.9 lb ft
Surge Tank Retaining Bolt And Nut | 8 N·m | 14.8 lb in
Thermostat Housing Bolts | 23 N·m | 71 lb ft
Transaxle Oil Cooler And Line Retaining Bolt | 10 N·m | 17 lb in
Water Pipe Retaining Bolt (M6) | 9 N·m | 88.5 lb in
Water Pipe Retaining Bolt (M8) | 20 N·m | 14.8 lb ft
Water Pump Tightening Bolt | 11 N·m | 97.4 lb in