For 1990-2009 cars

### Removal Procedure

1. Remove the engine undercover shield. Refer to Engine Shield Replacement.
2. Drain the engine oil.
3. Remove the oil pan. Refer to Oil Pan Replacement.
4. Remove the oil strainer. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement.
5. Remove the crankshaft balancer.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the crankshaft balancer and tighten the bolts to 55 N·m (46 lb ft).

Note: Do not disassemble the crankshaft balancer. Otherwise, the engine and body may be able to vibrate.

2. Turn the crankshaft and align the crankshaft balancer 3-point on the gears.
3. Install the oil strainer. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement.
4. Install the oil pan. Refer to Oil Pan Replacement.
5. Fill with engine oil.
6. Install the engine undercover shield. Refer to Engine Shield Replacement.