For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to . Battery Negative Cable Disconnection and Connection .
2. Disconnect the electrical connector.
3. Press the button on the docking station cradle.
4. Remove the docking station cradle from the docking station.
5. Remove the screws and slide the docking station.
6. Remove the docking station from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the docking station with the screws.

Tighten
Tighten the docking station screws to 2 N·m (18 lb in).

2. Install the docking station cradle to the docking station.
3. Connect the electrical connector.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .