For 1990-2009 cars

## Underhood Electrical Center or Junction Block Replacement HP7

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the junction block cover.

1 | Battery Positive Cable to Junction Block Bolt (Qty: 3)

#### Procedure

1. Remove battery cable nut on junction block and remove batter cable.
2. Remove the junction by releasing the tabs.

2 | Underhood Electrical Center or Junction Block