For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transaxle brace to engine oil pan bolts (2).
3. Remove the transaxle brace to transaxle bolt (1).
4. Remove the transaxle brace (3).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transaxle brace (3).
2. Install the transaxle brace bolts (1, 2), and tighten to 50 N·m (37 lb ft).
3. Lower the vehicle.