For 1990-2009 cars

### Removal Procedure

Before disconnecting the reservoir tank hose, remove the clutch fluid from the reservoir tank.

1. Remove the locking clip from the clutch pedal.
2. Remove the push rod from the clutch pedal.
3. Disconnect the hose clamp on the master cylinder.
4. Disconnect the master cylinder hose.
5. Remove the master cylinder pipe.
6. Remove the clutch master cylinder nuts.
7. Remove the clutch master cylinder.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the clutch master cylinder and clutch master cylinder nuts and tighten to 23 N·m (17 lb ft).
2. Connect the pipe to the master cylinder.
3. Connect the master cylinder hose.
4. Connect the hose clamp on the master cylinder.
5. Install the push rod to the clutch pedal.
6. Install the locking clip to the clutch pedal.
7. Bleed the air. Refer to Hydraulic Clutch Bleeding.
8. Fill the reservoir with clutch fluid up to the proper level.