For 1990-2009 cars

### Removal Procedure

1. Clean any dirt or debris away from the transaxle fluid plug/level indicator area.
2. Remove the transaxle fluid level indicator bolt from the transaxle.
3. Remove the transaxle fluid level indicator from the transaxle.
4. Wipe away any transaxle fluid from the fluid level indicator (2).

### Installation Procedure

1. Install the transaxle fluid level indicator onto the transaxle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transaxle fluid level indicator bolt (1) to the transaxle.

Tighten
Tighten the bolt to 10 N·m (89 lb in).