For 1990-2009 cars

Callout | Component Name
--- | ---
Important:

• | Inspect all components or sub-components and perform any repair procedure necessary to fix the damage. If the damage cannot be repaired, replace the component or sub-component as indicated.

• | Clean all components in cleaning solvent and air dry.

• | The transfer case input shaft and transfer case rear output drive shaft is not serviced. If damage cannot be repaired, the transfer case must be replaced.

1 | Transfer Case Input Shaft Gear Important: Inspect for pitting, excessive wear, or damage.
2 | Transfer Case Rear Output Drive Shaft Gear Important: Inspect for pitting, excessive wear, or damage.
3 | Transfer Case Input Shaft Bearing Assembly Important: Inspect bearings for roughness, spalling, or pitting.
4 | Transfer Case Rear Output Drive Shaft Bearing Assembly Important: Inspect bearings for roughness, spalling, or pitting.