For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Mounting Bracket Bolts | 37 N·m | 27 lb ft
Accessory Pedal Module Retaining Bolts | 9 N·m | 80 lb in
Camshaft Position Sensor Bolts | 8 N·m | 71 lb in
Crankshaft Position Sensor Retaining Bolt | 8 N·m | 71 lb in
Electronic Ignition System Ignition Coil Retaining Bolts | 10 N·m | 89 lb in
Engine Control Module Bracket Retaining Nuts | 15 N·m | 11 lb ft
Engine Coolant Temperature Sensor Bolt | 20 N·m | 15 lb ft
Evaporative Emission Canister Bracket Nuts | -- | --
Evaporative Emission Canister Purge Solenoid Bracket Bolt | 10 N·m | 89 lb in
Exhaust Gas Recirculation Valve Retaining Bolts | 30 N·m | 22 lb ft
EGR Valve Adapter Retaining Bolt (Left) | 20 N·m | 15 lb ft
EGR Valve Adapter Retaining Bolt (Upper and Right) | 20 N·m | 15 lb ft
Fuel Rail Retaining Bolts | 25 N·m | 18 lb ft
Fuel Tank Strap Retaining Bolts | 20 N·m | 15 lb ft
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure Sensor Retaining Bolt | 4 N·m | 35 lb in
Oxygen Sensor Bolt | 50 N·m | 37 lb ft
Rear A/C Compressor Mounting Bracket Bolts | 23 N·m | 17 lb ft
Throttle Body Retaining Nuts | 10 N·m | 89 lb in