For 1990-2009 cars

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the floor console. Refer to Console Replacement .
3. Disconnect the electrical connector.
4. Remove the cellular telephone module from the bracket.

### Installation Procedure

Important: Perform the programming when the cellular telephone module is being replaced.

1. Install the cellular telephone module into the bracket.
2. Connect the electrical connector.
3. Install the floor console. Refer to Console Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .