For 1990-2009 cars

### Removal Procedure

1. Remove the bolts securing the rear portion of the rear seat to the floor.
2. Remove the seat.

### Installation Procedure

1. Install the rear seat cushion by inserting the metal loops into the rear retaining brackets and pressing the front of the seat cushion down.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts into the rear portion of the rear seat.

Tighten
Tighten the rear seat-to-floor bolts to 45 N·m (33 lb ft).