For 1990-2009 cars

Caution: The steering column must be in the LOCK position before disconnecting the following components:

• | The steering column

• | The steering shaft coupling

• | The intermediate shaft

• | The lower steering shaft

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.