For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery negative cable and then disconnect the battery positive cable.
2. Loosen the nuts that fasten the battery hold-down bar bracket.
3. Remove the battery hold-down bar bracket with the nuts attached.
4. Remove the battery from the battery tray.

### Installation Procedure

1. Install the battery.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the battery hold-down bar bracket.

Tighten
Tighten the battery hold-down bar bracket retaining nuts to 4 N·m (35 lb in).

3. Connect the positive battery cable.
4. Connect the negative battery cable.