For 1990-2009 cars

## Front Side Door Lock Replacement C100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the screws and the front door lock.
4. Disconnect the lock rods.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front door lock with the screws.

Tighten
Tighten the front door lock bolt to 8 N·m (71 lb in).

4. Install the water deflector. Refer to Door Water Deflector Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .

## Front Side Door Lock Replacement C105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the screws and the front door lock.
4. Disconnect the lock rods.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front door lock with the screws.

Tighten
Tighten the front door lock bolt to 8 N·m (71 lb in).

4. Install the water deflector. Refer to Door Water Deflector Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .