For 1990-2009 cars

### Removal Procedure

1. Drain the engine oil.
2. Remove the oil filter housing drain bolt with washer and drain the engine oil in the oil filter housing.
3. Remove the oil filter cap with the O-ring.

Important: Check the engine oil maintenance interval and replace the engine oil filter according to the interval. Also, you can check the engine oil remaining life in the scan tool.

4. Remove the oil filter.
5. Remove the oil filter housing adapter plate.
6. Remove the oil filter housing with the O-ring.

### Installation Procedure

1. Install the engine oil filter housing with a new O-ring.
2. Install the oil filter housing adapter plate.

Tighten
Tighten the oil filter housing adapter plate to 40 N·m (29.5 lb ft).

3. Install the engine oil filter and cap with a new O-ring.

Tighten
Tighten the engine oil filter cap to 25 N·m (18.4 lb ft).

4. Install the oil filter housing drain bolt with washer.