For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air cleaner outlet duct. Refer to Air Cleaner Assembly Replacement.

1 | Transmission Fluid Cooler Pipe Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Sealing Washer Tip Remove and discard the sealing washer.
3 | Transmission Fluid Cooler Inlet Hose

#### Procedure

1. Disconnect the transmission line from the radiator and transmission. Refer to Transmission Fluid Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection.
2. Note the routing of the transmission line to ensure proper installation.
3. Remove the transmission line from the clips securing the line to the transmission and fan shroud.
4. Inspect the transmission fluid level. Refer to Transmission Fluid Check.