For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the cap and the nuts from the strut upper area.
3. Remove the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
4. Remove the brake hose bracket bolt.
5. Remove the stabilizer link to strut upper nut.
6. Remove the strut bracket to knuckle bolts and nuts.
7. Remove the strut assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the strut assembly to the knuckle with the bolts and nuts and tighten to 180 N·m (133 lb ft).
2. Install the brake hose bracket to the strut with the bolt and tighten to 15 N·m (11 lb ft).
3. Install the nuts to the strut and tighten to 30 N·m (22 lb ft).
4. Install the cap to the top of the strut.
5. Install the stabilizer link to strut upper nut and tighten to 65 N·m (48 lb ft).
6. Install the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
7. Measure the wheel alignment. Adjust the wheel alignment if necessary. Refer to Wheel Alignment Measurement.
8. Lower the vehicle.