For 1990-2009 cars

Connector 1: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 2: | Inflatable Restraint Steering Wheel Module Coil X2

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BN | 180 | Remote CD/Cassette Player Supply Voltage (C100)
B | 0.35 L-GN | 1011 | Remote Radio Control Signal (C105)
C | 0.35 GY | 1884 | Cruise Controls Switch Signal (C100)
C | 0.35 BK | 351 | Ground (C105)
D | 0.35 L-GY | 902 | Handset Volume Control Ground (C100/LHD)
E | 0.35 L-GN | 1011 | Remote Radio Control Signal (C100)
E | 0.35 PK | 1444 | 12-Volt Reference (C105)
F | 0.35 PK | 1444 | 12-Volt Reference (C100)
F | 0.35 YE/BK | 9088 | I/P Lamp Supply Voltage (C105)
G | 0.35 BU/WH | 901 | Handset Volume Control Supply (C100/LHD)
H | -- | -- | Not Used
J | 0.35 BK | 350 | Ground
K | 0.35 TN | 28 | Horn Relay Control

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BN | 180 | Remote CD/Cassette Player Supply Voltage (C100)
B | 0.35 L-GN | 1011 | Remote Radio Control Signal (C105)
C | 0.35 GY | 1884 | Cruise Controls Switch Signal (C100)
C | 0.35 BK | 351 | Ground (C105)
D | 0.35 L-GY | 902 | Handset Volume Control Ground (C100/LHD)
E | 0.35 L-GN | 1011 | Remote Radio Control Signal (C100)
E | 0.35 PK | 1444 | 12-Volt Reference (C105)
F | 0.35 PK | 1444 | 12-Volt Reference (C100)
F | 0.35 YE/BK | 9088 | I/P Lamp Supply Voltage (C105)
G | 0.35 BU/WH | 901 | Handset Volume Control Supply (C100/LHD)
H | -- | -- | Not Used
J | 0.35 BK | 350 | Ground
K | 0.35 TN | 28 | Horn Relay Control