For 1990-2009 cars

#### Body Control Module (BCM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Wiper Test | Front Wiper Relay | The wiper switch has to be in the Low position for this output control to function. The BCM actuates the Wiper relay when ON is selected. The front wiper should operate at low speed.
Wiper Test | Rear Wiper Relay | The wiper switch has to be in the Low position for this output control to function. The BCM actuates the Wiper relay when ON is selected. The rear wiper should operate at low speed.