For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Support the engine assembly using DW-110-060 fixture .
2. Remove the transaxle front mount-to-transaxle through bolt.
3. Remove the transaxle front mount retaining bolts from the transaxle.
4. Remove the transaxle front mount assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transaxle front mount assembly and tighten the retaining bolts to 50 N·m (36.9 lb ft).

Note: Before tightening the transaxle front mount through bolt swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

2. Install the transaxle front mount through bolt and tighten to 90 N·m (66 lb ft).
3. Remove the support fixture DW-110-060 fixture .