For 1990-2009 cars

Connector 1: | Fuse Block - I/P - Label
Connector 2: | Fuse Block - I/P X1
Connector 3: | Fuse Block - I/P X2
Connector 4: | Fuse Block - Underhood Auxiliary Label (Diesel)
Connector 5: | Fuse Block - Underhood Label
Connector 6: | Fuse Block - Underhood X1
Connector 7: | Fuse Block - Underhood X2
Connector 8: | Fuse Block - Underhood X3

### Fuse Block - I/P - Label

#### Fuse Block - I/P - Label Usage

Fuse | Rating | Description
--- | --- | ---
F1 | 20A | Power Window Main Switch, Sunroof Module
F2 | 20A | Power Window Main Switch
F3 | 10A | Front Washer Pump Relay
F4 | -- | Not Used
2A | BCM, Contact Coil (C105/Short Body)
F5 | 10A | SDM
F6 | 10A | SDM
F7 | -- | Not Used
F8 | 10A | Rear Fog Lamp Relay
F9 | 10A | Rear Fog Lamp Relay, Fuel Pump, Fuel Tank Level Sensor, ECM Mirror, Clutch Switch
F10 | 10A | Radio, Clock
Radio (C105/Short Body)
F11 | 10A | BCM
F12 | 2A | Ignition Switch, Immobilizer
F13 | 10A | Instrument Cluster, Driver Information Center, Passenger Seat Belt Indicator
Instrument Cluster, I/P Center Switch (C105/Short Body)
F14 | 15A | BCM, XBCM
BCM, XBCM, Trailer Kit Inline (C105/Short Body)
F15 | 10A | Power Steering Control Module
Power Steering Control Module, SI-ECM, Head Lamp (C105/Short Body)
F16 | 20A | BCM
F17 | 15A | Outside Rearview (OSRV) Mirror Heating Relay
10A | Outside Rearview (OSRV) Mirror Heating Relay (C105/Short Body)
F18 | 10A | Manual HVAC Control, Auto HVAC Control, Air Quality Sensor, Blower High Relay, Object Detection Module, Engine Auxiliary Fuse Block (PTC Relay)
Manual HVAC Control, Auto HVAC Control, Air Quality Sensor, Blower High Relay, Object Detection Module, Engine Auxiliary Fuse Block (PTC Relay), Heated Seat Unit (C105/Short Body)
F19 | 15A | Manual HVAC Control, Auto HVAC Control, DLC
F20 | 10A | Lift Gate Glass Relay
-- | Not Used (C105/Short Body)
F21 | -- | Not Used
10A | Tail Lamp Right, Head Lamp Right, Park Lamp Right (C105/Short Body)
F22 | -- | Not Used
10A | Liftgate Latch Assembly (C105/Short Body)
F23 | -- | Not Used
10A | Trailer Inline, Trailer Kit Inline (C105/Short Body)
F24 | 15A | BCM
F25 | 10A | XBCM
XBCM, Trailer Kit Inline, Power Sounder (C105/Short Body)
F26 | 15A | BCM
F27 | 15A | Front Fog Relay
F28 | 15A | Instrument Cluster, Clock, Radio, RFA Receiver, Driver Information Center
Instrument Cluster, I/P Center Switch, Radio, RFA Receiver, Driver Information Center, UHP Communication Box, Object Detection Module, Power Sounder, Intrusion Sensor, Inclination Sensor (C105/Short Body)
F29 | 15A | TCM
F30 | 20A | Heated Seat Switch
-- | Not Used (C105/Short Body)
F31 | 15A | BCM
F32 | 20A | Auxiliary Power Outlet - Cargo
Auxiliary Power Outlet - Cargo, Trailer Inline, Trailer Kit Inline (C105/Short Body)
F33 | 20A | Cigar Lighter
F34 | 20A | Auxiliary Power Outlet - Cargo
Auxiliary Power Outlet - Cargo, Trailer Relay Module, Trailer Kit Inline (C105/Short Body)
F35 | 15A | BCM
F36 | 15A | Door Dead Lock Relay
Door/Fuel Unlock Relay (C105/Short Body)
F37 | 10A | Power Window Switch
F38 | 20A | Door Lock/Unlock Relay
F39 | 10A | Mirror Control Switch, Folding Mirror Unit
Mirror Control Switch, Folding Mirror Unit, I/P Center Switch, Sun Roof Module (C105/Short Body)

### Fuse Block - I/P X1

#### Connector Part Information

- OEM: TYCO 0-1743134-2
- Service: N/A
- Description: 60-Way F Unsealed

#### Fuse Block - I/P X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YE | -- | Accessory Voltage
3-9 | -- | -- | Not Used
10 | PK | -- | Run/Crank Ignition 1 Voltage
11 | PK | -- | Run/Crank Ignition 1 Voltage
12 | PK | -- | Run/Crank Ignition 1 Voltage
13 | -- | -- | Not Used
14 | RD/WH | -- | Battery Positive Voltage
15-16 | -- | -- | Not Used
17 | YE | -- | Accessory Voltage
18 | YE | -- | Accessory Voltage
19 | PK | -- | Run/Crank Ignition 1 Voltage
20-21 | -- | -- | Not Used
22 | RD/WH | -- | Battery Positive Voltage
23-24 | -- | -- | Not Used
25 | PK | -- | Run/Crank Ignition 1 Voltage
26 | YE | -- | Run/Crank Ignition 1 Voltage
27-28 | -- | -- | Not Used
29 | RD/WH | -- | Battery Positive Voltage
30 | RD/WH | -- | Battery Positive Voltage
31 | -- | -- | Not Used
32 | PK | -- | Run/Crank Ignition 1 Voltage
33-34 | -- | -- | Not Used
35 | RD/WH | -- | Battery Positive Voltage
36-37 | -- | -- | Not Used
38 | RD/WH | -- | Battery Positive Voltage
39-40 | -- | -- | Not Used
41 | RD/WH | -- | Battery Positive Voltage
42 | RD/WH | -- | Battery Positive Voltage
43 | BN | -- | Run Ignition 3 Voltage
44-45 | -- | -- | Not Used
46 | RD/WH | -- | Battery Positive Voltage
47-48 | -- | -- | Not Used
49 | RD/WH | -- | Battery Positive Voltage
50 | RD/WH | -- | Battery Positive Voltage
51-53 | -- | -- | Not Used
54 | RD/WH | -- | Battery Positive Voltage
55-56 | -- | -- | Not Used
57 | RD/WH | -- | Battery Positive Voltage
58 | RD/WH | -- | Battery Positive Voltage
59 | BN | -- | Run Ignition 3 Voltage
60 | BN | -- | Run Ignition 3 Voltage

### Fuse Block - I/P X2

#### Connector Part Information

- OEM: TYCO 0-1743134-3
- Service: N/A
- Description: 60-Way F 110/250/375 Unsealed

#### Fuse Block - I/P X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | RD/WH | -- | Battery Positive Voltage
4 | OG | -- | Rear For Lamp Supply Voltage
5-6 | -- | -- | Not Used
7 | RD/WH | -- | Battery Positive Voltage
8 | BN | -- | Run Ignition 3 Voltage
9 | -- | -- | Not Used
10 | PK | -- | Run/Crank Ignition 1
11 | WH | -- | Rear Defog Relay Control
12 | PK | -- | Lift Glass/Trunk Exterior Release Signal
13 | RD/WH | -- | Battery Positive Voltage
14 | -- | -- | Not Used
15 | RD/WH | -- | Battery Positive Voltage
16 | BN | -- | Run Ignition 3 Voltage
17 | YE | -- | Accessory Voltage
18 | PK | -- | Run/Crank Ignition 1 Voltage
19 | PK | -- | Run/Crank Ignition 1 Voltage
20 | OG | -- | Windshield Washer Pump Control
21 | RD/WH | -- | Battery Positive Voltage
22-23 | -- | -- | Not Used
24 | BN | -- | Run Ignition 3 Voltage
25 | YE | -- | Run/Crank Relay Coil Control
26 | PK | -- | Run/Crank Ignition 1 Voltage
27 | BN | -- | Lift Glass/Trunk Motor Release Control
28 | RD/WH | -- | Battery Positive Voltage
29-30 | -- | -- | Not Used
31 | BN | -- | Rap Relay Coil Control
32 | PK | -- | Run/Crank Ignition 1 Voltage
33 | YE | -- | Rear Fog Lamp Relay Control
34 | RD/WH | -- | Battery Positive Voltage
35 | -- | -- | Not Used
36 | RD/WH | -- | Battery Positive Voltage
37 | YE | -- | Accessory Voltage
38 | YE | -- | Power Supply
49 | RD/WH | -- | Battery Positive Voltage
40-41 | -- | -- | Not Used
42 | RD/WH | -- | Battery Positive Voltage
43 | OG | -- | --
44 | BN | -- | Signal Ground
45 | YE | -- | Accessory Voltage
46 | -- | -- | Not Used
47 | GY | -- | Door Lock Actuator Lock Control
48 | RD/WH | -- | Battery Positive Voltage
49 | BN | -- | Door Lock Actuator Unlock Control
50 | -- | -- | Not Used
51 | RD/WH | -- | Battery Positive Voltage
52 | -- | -- | Not Used
53 | YE | -- | Accessory Voltage
54 | -- | -- | Not Used
55 | BN | -- | Driver Door Lock Actuator Unlock Control
56 | L-GN | -- | Left Front Door Lock Relay Control
57 | BK | -- | Ground
58 | PK/BK | -- | Engine Main Relay Fused Control (2)
59-60 | -- | -- | Not Used

### Fuse Block - Underhood Auxiliary Label (Diesel)

#### Fuse Block - Underhood Auxiliary -- Label Usage (Diesel)

Fuse | Rating | Description
--- | --- | ---
Af1 | 60A | Glow Plug Control Unit
Af2 | 30A | Fuel Filter Heater Relay
Af3 | 40A | PTC-1 Relay
Af4 | 40A | PTC-2 Relay
Af5 | 40A | PTC-3 Relay

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

Fuse | Rating | Description
--- | --- | ---
Ef1 | 20A | Rear Wiper Motor
Ef2 | 60A | I/P Fuse Block (Battery Main)
Ef3 | 40A | I/P Fuse Block (IGN II), Blower Motor
Ef4 | 40A | ABS Module
Ef5 | 20A | Starter Relay
Ef6 | 30A | Liftgate Defogger
Ef7 | 40A | I/P Fuse Block (ACC/RAP Relay, Run/Crank Relay)
Ef8 | 30A | Cooling Fan Auxiliary
Ef9 | 30A | Cooling Fan Main
Ef10 | 20A | ECM
Ef11 | 15A | 2.0L: Throttle Plate Actuator, Boost Pressure Actuator, CMP Sensor 2.4L: Canister Purge Solenoid, LEGR Valve, CMP Sensor 3.2L: Ignition Coil, Injector (#2, 4, 6)
Ef12 | 15A | 2.0L: ECM 2.4L: Front and Rear HO2S 3.2L: HO2S, VIM, CAM Phaser Intake/Exhaust, Canister Purge Solenoid
Ef13 | 10A | Starter Relay, Main Relay
Starter Relay, Main Relay, ECM (C105/Short Body)
Ef14 | 10A | A/C Compressor Relay
Ef15 | 15A | 2.0L: Glow Plug Control Unit, Cooling Fan (Auxiliary, Main, Control), A/C COMP Relay, Engine Fuse Block Auxiliary 2.4L: Injector, Cooling Fan (AUX., Main Control), A/C Comp. Relay 3.2L: Ignition Coil, Injector (#1, 3, 5), Cooling Fan (Auxiliary, Main, Control) A/C Compressor Relay
Ef16 | 15A | AWD Control Module
Ef17 | 15A | Fuel Pump Relay
Ef18 | 20A | ABS Module, Oil Feeding Connector
Ef19 | -- | Not Used
20A | Heated Seat Control Unit (C105/Short Body)
Ef20 | 15A | Brake Switch
Ef21 | 25A | Cooling Fan Control Relay
Ef22 | 15A | Horn Relay
Ef23 | 30A | Power Seat and Heated Seat Switch Power Seat Test Connector
Ef24 | 15A | Head Lamp Left, Tail Lamp Left, Turn/Park Lamp Left, License Lamp
Ef25 | 20A | Sunroof Module
Ef26 | 15A | Head Lamp Right, Mirror Control Switch
Head Lamp Right, Light Switch, SI-ECM (C105/Short Body)
Ef27 | 15A | Head Lamp Left
Ef28 | 15A | Head Lamp
Ef29 | 15A | FRT Fog Lamp Relay
Ef30 | 10A | Headlamp Left, Tail Lamp Left
Headlamp Left, Tail Lamp Left, Park Lamp Left, License Lamp Relay (C105/Short Body)
Ef31 | 10A | Headlamp Right, Tail Lamp Right
Trailer Inline, Trailer Kit Inline (C105/Short Body)
Ef32 | 15A | TCM
Ef33 | 20A | Headlamp Washer
Ef34 | -- | Not Used
Ef35 | 20A | Not Used
Ef36 | 25A | Not Used
Ef37 | 10A | Not Used
Ef38 | 15A | Not Used

### Fuse Block - Underhood X1

#### Connector Part Information

- OEM: TYCO 0-1743130-2
- Service: N/A
- Description: 55-Way Block Assembly Unsealed

#### Fuse Block - Underhood X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 532 | Cooling Fan Motor Supply Volt (2)
2 | 0.35 PK/BK | 5291 | Ignition 1 Voltage
3 | 0.35 PK/BK | 5291 | Ignition 1 Voltage
4 | 0.35 PK/BK | 5291 | Ignition 1 Voltage
5 | -- | -- | Not Used
6 | 0.5 RD/WH | 40 | Battery Positive Voltage (LD9)
6 | 0.5 BK/WH | 251 | Ground (LLW/LU1)
7 | 2 PU | 6 | Starter Solenoid Crank Voltage
8 | 0.35 YE | 447 | Starter Relay Coil Control
9-10 | -- | -- | Not Used
11 | 0.35 PK/BK | 5292 | Ignition 1 Voltage (LLW/LU1)
12 | 0.35 PK/BK | 5292 | Ignition 1 Voltage (LD9/LLW)
13 | 0.35 PK/BK | 5292 | Ignition 1 Voltage (LD9/LLW)
14 | 0.35 PK/BK | 5292 | Ignition 1 Voltage (LD9/LLW)
15 | -- | -- | Not Used
16 | 0.35 PK/BK | 5293 | Ignition 1 Voltage (LD9)
17 | 0.35 PK/BK | 5293 | Ignition 1 Voltage
18 | 0.35 PK/BK | 5293 | Ignition 1 Voltage
19 | -- | -- | Not Used
20 | 0.35 PK/BK | 5290 | Ignition 1 Voltage
21 | 0.35 PK/BK | 5290 | Ignition 1 Voltage (LLW/LU1)
22 | 0.35 L-BU | 409 | Cooling Fan Motor Supply Volt (1)
23-24 | -- | -- | Not Used
25 | 0.35 D-GN | 59 | A/C Comp Clutch Supply Volt
26 | 0.35 PK/BK | 5293 | Ignition 1 Voltage
27 | 0.35 PK/BK | 5293 | Ignition 1 Voltage (LD9/LU1)
28 | 0.5 BK | 150 | Ground
29 | -- | -- | Not Used
30 | 0.35 D-GN | 335 | Low Speed Cooling Fan Relay Control
31-32 | -- | -- | Not Used
33 | 0.35 WH | 504 | Cooling Fan Motor Low Reference
34 | 0.35 YE | 772 | Trans PSN Switch B2 Signal (M98)
35 | 0.35 PK | 539 | Ignition 1 Voltage
36 | 0.35 RD/WH | 40 | Battery Positive Voltage (LD9/LU1)
37 | 0.35 RD/WH | 40 | Battery Positive Voltage (LD9)
38 | -- | -- | Not Used
39 | 0.35 BK/WH | 251 | Signal Ground
40-41 | -- | -- | Not Used
42 | 0.35 BN | 41 | Ignition 3 Voltage (LLW)
43 | 0.35 BN/WH | 771 | Trans PSN Switch B1 Signal (M98)
44 | 0.35 WH | 776 | Trans PSN Switch PB Signal (M98)
45 | 0.35 PK | 539 | Run/Crank Ignition 1 Voltage
46 | 0.35 D-GN/WH | 459 | A/C Comp Clutch Relay Control
47 | -- | -- | Not Used
48 | 0.35 D-GN/WH | 465 | Fuel Pump Primary Relay Control
49-50 | -- | -- | Not Used
51 | 0.35 GY | 773 | Trans PSN Switch B3 Signal
52 | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control (LD9)
52 | 0.35 WH/BK | 910 | PTC Request Signal (LLW)
53 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
54 | 0.35 PK | 539 | Run/Crank Ignition 1 Voltage
55 | 0.35 D-BU | 473 | High Speed Cooling Fan Relay Control
56 | -- | -- | Not Used

### Fuse Block - Underhood X2

#### Connector Part Information

- OEM: TYCO 0-1743126-2
- Service: N/A
- Description: 60-Way Block Assembly Unsealed

#### Fuse Block - Underhood X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 120 | Fuel Pump Supply Voltage
2 | 0.35 PU | 92 | Windshield Wiper Motor High Speed
3 | -- | -- | Not Used
4 | 0.35 BN/WH | 41 | Ignition 3 Voltage
5 | 0.35 BN/WH | 771 | Transmission PSN Switch B1 Signal (M98)
6 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
7 | 0.35 PK | 539 | Ignition 1 Voltage
8 | 0.35 RD/WH | 2440 | Battery Positive Voltage
9 | 0.35 RD/WH | 840 | Battery Positive Voltage
10 | 0.35 RD/WH | 540 | Battery Positive Voltage
11 | -- | -- | Not Used
12 | 0.35 D-GN | 95 | Windshield Washer Switch Signal
13 | -- | -- | Not Used
14 | 0.35 YE | 772 | Transmission PSN Switch B2 Signal (M98)
15 | 0.35 WH | 776 | Transmission PSN Switch PB Signal (M98)
16 | 0.35 WH | 2282 | Headlamp Washer Relay Control
17 | 0.35 RD/WH | 640 | Battery Positive Voltage (U88)
18 | 0.35 BN | 860 | Front Windshield Wiper Switch High Signal
19 | 0.35 RD/WH | 2140 | Battery Positive Voltage (AWD)
20 | 0.35 GY | 773 | Transmission PSN Switch B3 Signal (M98)
21 | 0.35 WH/BK | 910 | PTC Request Signal (LLW)
22 | 0.35 BN | 28 | Horn Relay Control
23 | 0.35 RD/WH | 2540 | Battery Positive Voltage (VXC)
24 | 0.35 BN | 141 | Ignition 3 Voltage
25 | 0.35 PU/WH | 1970 | Headlamp Low Beam Relay Control
26 | 0.35 L-GN | 5486 | Run Relay Control
27-29 | -- | -- | Not Used
30 | 0.35 RD/WH | 2540 | Battery Positive Voltage (VXC)
31 | 0.35 PU | 709 | Left Park Lamp Supply Voltage
32 | 0.35 GN/WH | 1317 | Fog Lamp Relay Control
33 | 0.35 D-BU | 45 | Park Lamp Supply Voltage
34 | 0.35 L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage (-T90)
35 | 0.35 WH | 193 | Rear Defog Relay Control
36 | 0.35 GY | 91 | Windshield Wiper Switch Signal 2
37 | 0.35 RD/WH | 2040 | Battery Positive Voltage (LD9)
38 | 0.35 BN/WH | 312 | Right Headlamp Low Beam Supply Voltage
39 | 0.35 BN/WH | 309 | Right Park Lamp Supply Voltage
40 | 0.35 OG/BK | 645 | Low Reference
41 | 0.35 L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage (T90)
42 | 0.35 OG | 228 | Windshield Washer Pump Control
43 | 0.35 BN/WH | 1969 | Headlamp Relay Control
44 | 0.35 RD/WH | 240 | Battery Positive Voltage
45 | -- | -- | Not Used
46 | 0.35 L-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage (T90)
47 | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
48 | 0.35 RD/WH | 140 | Battery Positive Voltage
49 | 0.35 PU | 5531 | Hood Closed switch Signal
50 | 0.35 D-GN | 392 | Rear Window Washer Pump Control
51 | 0.35 RD/WH | 2240 | Battery Positive Voltageal
52 | 0.35 PU | 293 | Rear Defog Element Supply Voltage
53 | -- | -- | Not Used
54 | 0.35 D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage (-T90)
55 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal
56 | 0.35 RD/WH | 2340 | Battery Positive Voltage
57 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Signal
58 | -- | -- | Not Used
59 | 0.35 D-GN | 189 | Headlamp Leveling Motor Supply Voltage
60 | 0.35 RD/WH | 940 | Battery Positive Voltage

### Fuse Block - Underhood X3

#### Connector Part Information

- OEM: TYCO 1-1743130-3
- Service: N/A
- Description: 56-Way Block Assembly Unsealed

#### Fuse Block - Underhood X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN | 2609 | Park Lamps Supply Voltage
3 | 0.35 D-BU/WH | 1315 | Right Front T/Signal Lamp Supply Voltage
4 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal
5 | 0.35 BN | 41 | Run Ignition 3 Voltage
6 | 0.35 L-BU/WH | 1314 | Left Front T/Signal Lamp Supply Voltage
7 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal
8 | -- | -- | Not Used
9 | 0.35 D-GN | 392 | Rear Window Washer Pump
10 | -- | -- | Not Used
11 | 0.35 BN | 541 | Ignition 3 Voltage
12 | -- | -- | Not Used
13 | 0.35 D-GN/WH | 636 | Outside Ambient Air Temperature
14-15 | -- | -- | Not Used
16 | 0.35 PU | 5531 | Hood Closed Switch Signal
17 | 0.35 BN/WH | 6547 | Air Quality Sensor Low Reference
18 | 0.35 D-GN | 189 | HDLP Leveling Motor Supply Voltage
19 | -- | -- | Not Used
20 | 0.35 YE | 712 | Left HDLP Low Beam Supply Voltage
21 | -- | -- | Not Used
22 | 0.35 OG/BK | 645 | Sensor Low Reference
23 | -- | -- | Not Used
24 | 0.35 PU | 34 | Front Fog Lamp Supply
25 | -- | -- | Not Used
26 | 0.35 OG | 228 | Windshield Washer Pump Control
27 | 0.35 D-GN | 189 | HDLP Leveling Motor Supply Voltage
28-29 | -- | -- | Not Used
30 | 0.35 BN/WH | 312 | Right HDLP Low Beam Supply Voltage
31-33 | -- | -- | Not Used
34 | 0.35 D-GN/WH | 711 | Left HDLP High Beam Supply Voltage
35-36 | -- | -- | Not Used
37 | 0.35 BK | 150 | Ground
38 | -- | -- | Not Used
39 | 0.35 BN/WH | 709 | Left Park Lamp Supply Voltage
40-42 | -- | -- | Not Used
43 | 0.35 L-GN/BK | 311 | Right HDLP High Beam Supply Voltage
44 | -- | -- | Not Used
45 | 0.35 D-GN | 29 | HDRN Control
46 | 0.35 D-GN | 29 | HDRN Control
47-53 | -- | -- | Not Used
54 | 0.35 PU | 1197 | Headlamp Washer Pump Control
55-56 | -- | -- | Not Used