For 1990-2009 cars

## Liftgate Garnish Molding Replacement Upper

### Removal Procedure

1. Open the liftgate.
2. Remove the liftgate window upper garnish molding.

### Installation Procedure

1. Install the liftgate window upper garnish molding.
2. Close the liftgate.

## Liftgate Garnish Molding Replacement Side - C100/Long Body

### Removal Procedure

1. Open the liftgate.
2. Remove the liftgate window side garnish molding

### Installation Procedure

1. Install the liftgate window side garnish molding.
2. Close the liftgate.

## Liftgate Garnish Molding Replacement Side - C105/Short Body

### Removal Procedure

1. Open the liftgate.
2. Remove the liftgate window side garnish molding

### Installation Procedure

1. Install the liftgate window side garnish molding.
2. Close the liftgate.