For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the electrical connectors.
3. Remove the tail lamp assembly. Refer to Tail Lamp Replacement .
4. Remove any inoperative bulb.

### Installation Procedure

1. Install the replacement bulbs.
2. Install the tail lamp assembly. Refer to Tail Lamp Replacement .
3. Connect the electrical connectors.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .