For 1990-2009 cars

## Body Side Window Rear Garnish Molding Replacement C100/Long Body

### Removal Procedure

1. Remove the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear.
2. Remove the screws and the quarter window garnish molding.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the quarter window garnish molding with the screws and tighten to 2 N·m (18 lb in).
2. Install the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear.

## Body Side Window Rear Garnish Molding Replacement C105/Short Body

### Removal Procedure

1. Remove the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear.
2. Remove the screws and the quarter window garnish molding.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the quarter window garnish molding with the screws and tighten to 2 N·m (18 lb in).
2. Install the rear seat lower belts. Refer to Seat Belt Retractor Replacement - No. 1 Rear or Seat Belt Retractor Replacement - No. 2 Rear.