For 1990-2009 cars

#### Special Tools

• | J-23327 Clutch Spring Compressor

• | J-28585 Snap Ring Remover

• | J-23456 Booster and Clutch Pack Compressor

• | J-45184 Differential Bearing Race Installer

1. Remove the 1-2 reverse clutch backing plate retaining ring (622) using J-28585 remover .
2. Remove the following components:

• | The 1-2 reverse clutch backing plate (621)

• | The 6 1-2 reverse clutch fiber plates (620)

• | The 6 1-2 reverse clutch steel plates (619)

• | The 1-2 reverse clutch apply plate (618)

Note: Do not bend the 1-2 reverse clutch piston return spring assembly (601).

3. Place J-45184 installer (1) on the center of J-23456 compressor (2).
4. Place the transmission case cover (19) with the 1-2 reverse clutch piston assembly onto J-45184 installer (1).
5. Using J 23327-1 (3), which is the bridge part of J-23327 compressor , compress the 1-2 reverse clutch piston return spring assembly (601).
6. Remove the 1-2 reverse clutch piston return spring retaining ring (600) using snap ring pliers.
7. Remove the pressure from J-23456 compressor (2), remove J 23327-1 (3) and the 1-2 reverse clutch piston return spring assembly (601).
8. Remove all tools.

Warning: Wear safety glasses when using compressed air in order to prevent eye injury.

9. While pulling upward on the piston by hand, apply compressed air into the 1-2 reverse clutch fluid passage and remove the 1-2 reverse clutch piston (603).
10. Remove the 1-2 reverse clutch piston inner seal (602).
11. Remove the 1-2 reverse clutch piston outer seal (604).