For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the control solenoid valve and transmission control module assembly. Refer to Control Valve Body Replacement .
2. Perform the service fast learn adapt procedure. Refer to Service Fast Learn Adapts .

1 | Output Speed Sensor Bolt M6 x 18 Caution: Refer to Fastener Caution in the Preface section. Tip Tighten in specified sequence. Tighten
12 N·m (106 lb in)

2 | Output Speed Sensor