For 1990-2009 cars

#### Special Tools

J 28585 Snap Ring Remover

1. Remove the front internal gear thrust bearing (529).
2. Remove the low and reverse clutch plate retaining ring (518) from the transmission case assembly with J 28585 .
3. Remove the low and reverse clutch backing plate (520).
4. Remove the 5 low and reverse clutch fiber plate assemblies (516).
5. Remove the 4 low and reverse clutch steel plates (517).
6. Remove the low and reverse clutch apply plate (515).
7. Remove the front internal gear (526). The front internal gear thrust bearing assembly (519) and the thrust washer race (530) are on the back side of the front internal gear (526).