For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the coil spring. Refer to Coil Spring Replacement.
3. Remove the jounce bumper.

### Installation Procedure

1. Install the jounce bumper to the body panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the jounce bumper to the body panel hexagon bolt.

Tighten
Tighten the bolt to 15 N·m (11 lb ft).

3. Install the coil spring. Refer to Coil Spring Replacement.
4. Lower the vehicle.
5. Measure the wheel alignment. Adjust the wheel alignment if necessary. Refer to Wheel Alignment Measurement.