For 1990-2009 cars

## Starter Usage Gasoline Engines

Description | Specification
--- | ---
Unit | Standard
Type | -- | Permanent Magnet Gear Reduction (2.4L), PG 260D (3.2L)
Capacity | Kw | 1.4
No Load Test at 12 volts Condition Drive Pinion Speed | A | 90 MAX
Pinion Gear Speed | RPM | 2 600 MIN
Brush Length | mm (in) | 8.25
Armature Diameter | mm (in) | 45.5
Armature Runout | mm (in) | 0.08
Segment Home Depth | mm (in) | 0.6-1.0

## Starter Usage Diesel Engine

Description | Specification
--- | ---
Unit | Standard
Type | -- | PG 260NS
Capacity | Kw | 1.8
No Load Test at 12 volts Condition Drive Pinion Speed | A | 90 MAX
Pinion Gear Speed | RPM | 2 550 MIN