For 1990-2009 cars

#### Special Tools

• | J-41239-1A Cooler Line Seal Installer

• | J-45201 Cooler Line Seal Remover

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.

Warning: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

2. Place a drain pan or suitable container under the vehicle.
3. Remove the transaxle oil cooler line assembly nut from the transaxle.
4. Disconnect the transaxle oil cooler lines from the vehicle.

Note: Ensure that the J-45201 Remover is fully seated into the transaxle seal bore.

5. Insert the collet piece (2) of the J-45201 Remover into the cooler line seal.
6. Insert the forcing screw piece (1) of the J 45201 into the collet (2).
7. Tighten the forcing screw (1) until snug.
8. Thread the collar piece (1) of the J-45201 Remover onto the collet (3) until snug.
9. Turn the collar clockwise in order to remove the cooler line seal (87).
10. Discard the seal (87).
11. Clean the case bores for the cooler line seals.

### Installation Procedure

1. Insert a new transaxle cooler line seal into the case bore.
2. Remove the nub from the J-41239-1A Installer .
3. Install the nub of the J-41239-1A Installer on the transaxle cooler line seal.
4. Tap the new transaxle cooler line seal into the case bore.
5. Install the transaxle oil cooler line assembly to the transaxle.

Caution: Refer to Fastener Caution in the Preface section.

6. Install the transaxle oil cooler line assembly nut and tighten to 7 N·m (62 lb in).
7. Lower the vehicle.
8. Add fluid to the transaxle. Refer to Transmission Fluid Check.
9. Start the engine and check for leaks.