For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Bolt | 10 N·m | 89 lb in
Air Cleaner Assembly Bolt | 6 N·m | 53 lb in
Air Cleaner Inlet Duct Bolt | 6 N·m | 53 lb in
Air Cleaner Outlet Duct Clamp | 3 N·m | 27 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Evaporative Emission (EVAP) Canister Nut | 8 N·m | 71 lb in
Evaporative Emission (EVAP) Purge Solenoid Bracket Bolt | 10 N·m | 89 lb in
Fuel Fill Pipe Hose Clamp | 5 N·m | 44 lb in
Fuel Pressure Sensor | 15 N·m | 11 lb ft
Fuel Pump Flow Control Module Bolt | 10 N·m | 89 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Fill Pipe Bracket Nut | 4 N·m | 35 lb in
Fuel Tank Fill Pipe Housing to Fuel Tank Fill Pipe Screw | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 20 N·m | 15 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor Bolt | 23 N·m | 17 lb ft
Manifold Absolute Pressure (MAP) Sensor Bolt | 10 N·m | 89 lb in
Mass Air Flow (MAF)/Intake Air Temperature Sensor Bolt | 4 N·m | 35 lb in
Rear Brake Pipe Fitting to Brake Pressure Modulator Valve (BPMV) | 21 N·m | 16 lb ft
Rear Brake Pipe Fitting to Rear Brake Crossover Pipe Fitting | 18 N·m | 13 lb ft
Rear Brake Pipe Fitting to Rear Brake Hose Fitting | 18 N·m | 13 lb ft
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in