For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the front fender liner. Refer to Fender Liner Replacement .
4. Remove the front fender insulator.

### Installation Procedure

1. Install the front fender insulator.
2. Install the front fender liner. Refer to Fender Liner Replacement .
3. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.