For 1990-2009 cars

## Rear Seat Center Belt Buckle Replacement C100

### Removal Procedure

1. Fold the left rear seat forward.
2. Remove the screws and the rear seat outboard covers.
3. Remove the upper clip on the gas support assembly.
4. Disconnect the upper joint of the gas support assembly.
5. Remove the screws and the rear seat inboard cover.
6. Remove the bolt (1) and the seat belt buckle (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt buckle (2) and secure with bolt (1).

Tighten
Tighten the seat belt buckle bolt to 38 N·m (28 lb ft).

2. Install the rear seat inboard cover and sure with the screws.
3. Connect the upper joint of the gas support assembly and install the clip.
4. Install the rear seat outboard covers and secure with the screws.

## Rear Seat Center Belt Buckle Replacement C105

### Removal Procedure

1. Remove the screws and the compartment front tray.
2. Fold the left rear seatback forward.
3. Release the seat lock by pushing the lever forward on both seat legs.
4. Fold the rear left seat assembly forward.
5. Remove the bolt (1) and the seat belt buckle (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt buckle (2) and secure with bolt (1).

Tighten
Tighten the seat belt buckle bolt to 38 N·m (28 lb ft).

2. Reposition the left rear seat assembly.
3. Install the compartment front tray and the screws.