For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Disconnect the brake pipe from the brake hose.
3. Remove the brake hose retainer and remove the brake hose from the bracket.
4. Remove the rear brake hose from the rear upper control arm.
5. Remove the rear brake hose from the caliper.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear brake hose to the caliper and tighten the rear brake hose-to-caliper bolt to 32 N·m (24 lb ft).
2. Install the rear brake hose to the rear upper control arm.
3. Connect the rear brake pipe to the brake hose and install the hose retainer. Tighten the brake pipe line to fittings 16 N·m (12 lb ft).
4. Lower the vehicle.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding.
6. Check the brake system for leaks.