For 1990-2009 cars

## Fastener Tightening Specifications 2.4L and 3.2L

Application | Specification
--- | ---
Metric | English
Exhaust Front Pipe Mounting Bracket Bolt and Nut | 40 N·m | 30 lb ft
Exhaust Front Pipe To Underbody Catalytic Converter Nuts | 30 N·m | 22 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Front Muffler Heat Shields Nuts | 2.5 N·m | 22 lb in
Front Muffler To Rear Muffler Nuts | 40 N·m | 30 lb ft
Pup Converter Exhaust Front Pipe Nuts | 40 N·m | 30 lb ft
Pup Converter Upper Flange Nuts | 40 N·m | 30 lb ft
Rear Muffler Heat Shield Nuts | 2.5 N·m | 22 lb in
Underbody Catalytic Converter Heat Shield Nuts | 2.5 N·m | 22 lb in
Under Catalytic Converter To Front Muffler Nuts | 30 N·m | 22 lb ft

## Fastener Tightening Specifications 2.0L Diesel

Application | Specification
--- | ---
Metric | English
DPF Heat Shield Retaining Nut | 2.5 N·m | 22.1 lb in
Exhaust Front Pipe Nuts | 40 N·m | 29.5 lb ft
Exhaust Manifold Heat Shield Nut and Bolt | 20 N·m | 14.8 lb ft
Front Muffler Heat Shield Retaining Nut | 2.5 N·m | 22.1 lb in
Front Muffler-to-Rear Muffler Nut | 40 N·m | 29.5 lb ft
Pre-Catalyst Bracket Bolt | 40 N·m | 29.5 lb ft
Rear Muffler Heat Shield Retaining Nut | 2.5 N·m | 22.1 lb ft
Rear Muffler-to-Front Muffler Nut | 40 N·m | 29.5 lb ft