For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the stabilizer shaft clamp bolts.
3. Remove the insulators from the stabilizer shaft.

### Installation Procedure

1. Install the insulators the stabilizer shaft.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer shaft clamp bolts.

Tighten
Tighten the bolts to 70 N·m (52 lb ft).

3. Lower the vehicle.