For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

Note: Do not allow the stabilizer link ball stud to rotate while removing the link nut.

3. Remove the stabilizer link to strut nut.

Note: Do not allow the stabilizer link ball stud to rotate while removing the link nut.

4. Remove the stabilizer link to stabilizer bar nut.
5. Remove the stabilizer link.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: Do not allow the stabilizer link ball stud to rotate while installing the link nut.

1. Connect the stabilizer link to the strut and tighten to 85 N·m (63 lb ft).

Note: Do not allow the stabilizer link ball stud to rotate while installing the link nut.

2. Connect the stabilizer link to the stabilizer bar and tighten to 65 N·m (48 lb ft).
3. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
4. Lower the vehicle.