For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the rear console box.
3. Remove the rear console cover and disconnect the connector.
4. Remove the screws and heating mat switch.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the heating mat switch with the screws and tighten to 2 N·m (18 lb in).
2. Connect the connector and install the rear console cover.
3. Install the rear console box with the screws and tighten to 2 N·m (18 lb in).
4. Connect the negative battery cable.