For 1990-2009 cars

1. Remove the engine undercover shield. Refer to Engine Shield Replacement .
2. Drain the engine oil.
3. Remove the oil pan. Refer to Oil Pan Replacement .
4. Remove the oil strainer with washer.

### Installation Procedure

1. Install the oil strainer with washer.

Tighten

• | Tighten the oil strainer bolt to 11 N·m (97.4 lb in).

• | Tighten the oil strainer bracket bolt (bed plate outer bolt) to 35 N·m (25.8 lb ft).

2. Install the oil pan. Refer to Oil Pan Replacement .
3. Fill the engine with engine oil.
4. Install the engine undercover shield. Refer to Engine Shield Replacement .