For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the bolts and the rear impact bar.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear impact bar with the bolts.

Tighten
Tighten the rear impact bar bolts to 22 N·m (16 lb ft).

2. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .