For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the screws and the door speaker.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door speaker with the screws.

Tighten
Tighten the door speaker screws to 2 N·m (18 lb in).

3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .