For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the sunroof window. Refer to Sunroof Window Replacement.

1 | Sunroof Water Gutter Hook Arm

#### Procedure

1. Remember the location of the hole of curve on the panel which the water gutter hook arms hook into.

Release the sunroof water gutter hook arms from the sunroof frame on both sides.

2. Position the sunroof water gutter upright on both sides to location the tabs.

2 | Sunroof Water Gutter

#### Procedure

Remove the sunroof water gutter tab from the sunroof guide insert a flat blade tool and push inward on the tab to release it.