For 1990-2009 cars

### Removal Procedure

1. Turn the ignition to Off.
2. Remove the center console. Refer to Console Replacement .
3. Disconnect the yaw rate sensor connector.
4. Remove the yaw rate sensor attaching bolt.
5. Remove the yaw rate sensor.

### Installation Procedure

1. Install the yaw rate sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the yaw rate sensor attaching bolt.

Tighten
Tighten the nuts to 10 N·m (7 lb ft).

3. Connect the yaw rate sensor connector.
4. Install the center console. Refer to Console Replacement .