For 1990-2009 cars

## Liftgate Upper Applique Replacement C100/Long Body

### Removal Procedure

1. Open the liftgate.
2. Remove the nuts from the liftgate upper applique.
3. Close the liftgate.
4. Remove the liftgate upper applique from the vehicle.

### Installation Procedure

1. Position the upper applique to the liftgate.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the liftgate upper applique nuts.

Tighten
Tighten the liftgate upper applique nuts to 6 N·m (53 lb in).

## Liftgate Upper Applique Replacement C105/Short Body

### Removal Procedure

1. Open the liftgate.
2. Remove the nuts from the liftgate upper applique.
3. Close the liftgate.
4. Remove the liftgate upper applique from the vehicle.

### Installation Procedure

1. Position the upper applique to the liftgate.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the liftgate upper applique nuts.

Tighten
Tighten the liftgate upper applique nuts to 6 N·m (53 lb in).