For 1990-2009 cars

## Scan Tool Output Controls Except Holden

Table 1: | Body Control Module (BCM)
Table 2: | Instrument Panel Cluster (IPC)

#### Body Control Module (BCM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Interior Lamps | Output Control/Lamp Test | The body control module (BCM) turns the interior lamps ON when you select ON. The interior lamps should stay ON until commanded OFF.
I/P Illumination Lamps | Output Control/Lamp Test | The BCM turns the instrument panel illumination lamps on when you select ON. The illumination lamps should stay on until commanded OFF.
Transmission Range Indicator | Output Control/Lamp Test | The BCM turns the PRNDL indicators ON when you select ON. The PRNDL should stay ON until commanded OFF.

#### Instrument Panel Cluster (IPC)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Lamp and Gauge Check |  | The instrument panel cluster (IPC) illuminates the following indicators when you select ON:

• | ABS

• | Air Bag

• | BRAKE

• | Charge

• | Fasten Safety Belt

• | High Beam

• | Liftgate Ajar

• | Low Fuel

• | Low Oil Pressure

• | Low Traction

• | Reduced Engine Power

• | Security

• | Tire Pressure Monitor

• | Traction OFF

The IPC drives the following gages to maximum position when you select ON:

• | Engine Coolant Temperature Gage

• | Fuel Gage

• | Speedometer

• | Tachometer

The indicators should stay illuminated and all gages remain at maximum until commanded OFF. When commanded OFF, the indicators should turn OFF and all gages should remain at the minimum position until the test is exited or commanded ON.

## Scan Tool Output Controls Holden

#### Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
All Telltales Test | Body / IPC / Actuator Test | The instrument panel cluster (IPC) illuminates all the indicators.
Telltale Test | Body / IPC / Actuator Test | The instrument panel cluster (IPC) illuminates individual indicators.
Control Test | Body / IPC / Actuator Test | The instrument panel cluster (IPC) illuminates individual gauges.
Illumination Test | Body / IPC / Actuator Test | The BCM turns the instrument panel illumination lamps on when you select ON. The illumination lamps should stay on until commanded OFF.